Per-Model Setup

## Contents

1. Per-model setup: Only one model is viewed at any time, following a viewing protocol to collect gaze data for each.

## 1 Scene

### Model

### Booth

## 2 Collection Protocol

### 2.1 Calibration

### 2.2 Model Selection

### 2.3 Gaze Data Collection

### 2.4 Export Gaze Data

## 3 Gaze Data

### 3.1 CSV

### 3.2 Point Cloud

### 3.3 Preprocessing

### Gaussian Blur

### KD-Tree

### 3.4 Visualization

### Point Cloud

### Voxels